**Brand**

Venue

**Tagline**

**What it is**

Venue Tetra 6 RGBA LED Compact Wash Light

**Copy**

The Venue Tetra 6 RGBA LED Wash Light is designed for anyone who needs a professional quality color wash light. With six 4-watt quad-color LEDs and several internal operating modes, it provides a full palate of color control, including fourteen static colors, 20 standard chases, 20 sound-active chases, DMX control, Master/Slave capability, strobe, dimming, manual color mixing and more. Its double-yoke design provides precise aiming from stands, trusses and floors for complete venue coverage. For even more versatility, the Tetra 6 is compatible with DMX-512 operation, alongside controllers such as the Venue Tetra Control, and enjoy complete control in 3CH, 4CH, 5CH, or 6CH DMX mode. DMX In/Out jacks allow the use of multiple fixtures as well as master/slave functionality. Power linking capabilities minimize the need for outlets, and help keep cables clean and organized.

**Features**

• Features ultra-bright 4-watt LED bulbs

• RGBA color selection for more vivid colors and amber hues

• Compact design provides easy integration and versatility

• DMX compatibility ensures seamless system incorporation

• Set-it-and-forget-it standalone auto programming

• Built-in sound active mode with built-in microphone

• Static color mix control for ambient and up-lighting

• Power linking for up to 62 units at once

• Seamless compatibility with DMX-512 protocol, including controllers such as the Venue Tetra Control, for intuitive real-time operation.