**Brand**

Sterling

**What it is**

Sterling P10 Live Vocal Microphone

**Copy**

The Sterling Performance Series, P10 Instrument Microphone captures the midrange clarity and upper frequency presence with a full-frequency response that articulate acoustic instruments and robust guitar cabinet sounds demand. The P10’s premium-tuned frequency response mitigates the muddy, boxy, or even dull sounds that can be observed in other dynamic instrument mics. For the highest durability while on the road, the P10 uses a robust die-cast, zinc body that’s designed to be easy to handle on stage. A reinforced die-cast zinc head with reinforced mesh grill provides enhanced capsule protection, specially designed for long tours and demanding environments. Comes complete with mic clip and carry pouch.

**Features**

• Sterling Audio custom-tuned, Instrument performance capsule.

• Sterling Audio passive capsule suspension technology for ultra-low stage noise rejection and isolation.

• Cardioid polar pattern for off-axis noise rejection, and great SPL handling capability.

• Tour ready construction with die-cast zinc body and head assembly for demanding environments

• Transformer balanced XLR output connectivity for best isolation in Live venue environments.

**Specifications**

• Microphone Type: Instrument Microphone

• Transducer: Dynamic moving coil

• Polar Pattern: Cardioid  
• Frequency Response Range: 50Hz to 16kHz

• Sensitivity: 1.58 mV/Pa

• Output Impedance: 400 Ohms, Transformer Balanced

• Typical Load Impedance: >1000 Ohms  
• Product Length: 5.98 inches. (152mm)

• Product Weight: 8.6 oz. (243g)