**Brand**

Sterling

**What it is**

Sterling P20 Live Vocal Microphone

**Copy**

The Sterling P20 Vocal performance microphone captures the midrange clarity and full frequency response that performers demand. The P20’s premium-tuned frequency response mitigates the often boxy, muddy, or dull sounds that underperform in other vocal dynamic microphones. The cardioid polar pattern helps rejection of on-stage unwanted sounds and bleed to keep your vocals articulate. Its built-in windscreen provides protection from potential vocal plosives or wind noises if used in outdoor venues, and its enhanced capsule mounting and dampening design provided best-in-class isolation when handled. For the highest durability while on the road, the P20 uses a robust die-cast, zinc body that was ergonomically designed to be easy to handle on stage. A reinforced mesh grille provides enhanced capsule protection, specially designed for long tours and demanding environments. Comes complete with mic clip and carry pouch.

**Features**

• Sterling Audio custom-tuned, vocal performance capsule.

• Sterling Audio passive capsule suspension technology for ultra-low handling noise and isolation.

• Cardioid polar pattern for off-axis noise rejection, and great SPL handling capability.

• Ergonomically shaped body handle for a relaxed grip.

• Tour ready construction with die-cast zinc body and reinforced grill for demanding environments.

• Transformer balanced XLR output connectivity for best isolation in Live venue environments.

**Specifications**

• Microphone Type: Handheld Vocal Microphone

• Transducer: Dynamic moving coil

• Polar Pattern: Cardioid  
• Frequency Response Range: 50Hz to 16kHz

• Sensitivity: 2.24 mV/Pa

• Output Impedance: 400 Ohms, Transformer Balanced

• Typical Load Impedance: >1000 Ohms  
• Product Length: 10.6 oz. (301g)

• Product Weight: 7.24 inches. (184mm)