**Brand**

Harbinger

**Tagline**

Harbinger… Message Received.

**What It Is**

Harbinger L1202FX 12-Channel Mixer with Effects

**Model MFI# GC ID Enterprise#**

L1202FX J11557000000000 110448362 1401720417373

**Possible Headlines**

• It’s all About LvL’s

• LvL the Playing Field

• Step up to LvL

• The Next LvL is Here

**Harbinger L1202FX 12-Channel Mixer**

**100-Word**

The Harbinger L1202FX 12-Channel Mixer is an excellent choice for clear sound and flexible routing at an affordable price. Featuring four LvL Series mic preamps and four dual ¼” stereo inputs, these mixers provide plenty of routing options for home studio, stage or rehearsal. Enjoy high headroom and a 3-band EQ, plus functional features like assignable Aux In routing, 5-segment LED meters and built-in effects, including tap tempo delay. With clean sound and unparalleled control, you can now focus solely on creating and performing music. From recording to live to podcasting and more… Harbinger LvL has you covered.

**50-Word**

The 12-channel Harbinger L1202FX is an excellent mixer with an affordable price. Featuring four LvL Series mic preamps and four dual ¼” stereo inputs, you get plenty of routing options for home studio, stage or rehearsal. Enjoy high headroom, 3-band EQ, 5-segment LED meters and built-in effects, including tap tempo delay. From recording to live to podcasting and more… Harbinger LvL has you covered.

**25-Word**

The 12-channel L1202FX is an excellent mixer with an affordable price. Features include four LvL Series mic preamps, four dual ¼” stereo inputs, 3-band EQ per channel, 5-segment LED meters and built-in effects, including tap tempo delay.

**Features**

• 12-channel mixer with a variety of routing options

• 4 LvL Series ultra clean mic preamps with XLR and ¼” TRS balanced/unbalanced line input

• 4 TRS ¼” balanced/unbalanced stereo inputs with +4/-10dB sensitivity selection

• Built-in effects including tap tempo delay

• Versatile 3-Band EQ

• 75Hz high pass Filter on mic inputs

• Aux Send

• Full-size master fader

• Control room output for studio monitors

• 48V phantom power

• Input gain on mic preamps

• Input Signal/Peak indicator LED

• Pan/Balance controller per channel

• 5-Segment LED main mix meter

• RCA input and output

• Headphone outputs

• Robust external AC power supply

• Rugged metal chassis