**Brand**

Harbinger

**Tagline**

Message Received

**What it is**

Harbinger VaRi V1012 12” 400 Watt Powered Loudspeaker

**EID#**

x

**MFID#**

J46385

**GCID#**

112743372

**Possible Headlines**

• Reliable Portable Powerful

• Input Mixer, Power, Speaker — All in One Box

• Class-D Power in a Class by Itself

**100-Word**

The Harbinger VâRi V1012 12” powered loudspeaker is designed with 400 watts of clean, articulate Class-D amplification, bringing more power and exceptional sound to your band rehearsal, performance space, party or event. This robust 2-way speaker system features a 12” low frequency driver and a 1.35” compression driver plus a built-in 2-channel mixer with 2-band EQ. It also offers an advanced limiter with a clip indicator to protect your system and maintain pristine sound. And, with its XLR balanced line level output, you can link multiple speakers together for wall-to-wall coverage — perfect for anyone who needs venue-filling power and detail.

**50-Word**

The Harbinger VâRi V1012 12” powered loudspeaker is designed with 400 watts of clean, articulate Class-D amplification, bringing more power and exceptional sound to your band rehearsal, performance space, party or event. This robust 2-way speaker system features a 12” low frequency driver, 1.35” compression driver, 2-channel mixer, and a limiter with a clip indicator. And, with its XLR balanced line level output, you can link multiple speakers together for wall-to-wall coverage.

**25-Word**

The Harbinger VâRi V1012 12” powered loudspeaker is designed with 400 watts of clean, articulate Class-D amplification, bringing more power and exceptional sound to your band rehearsal, performance space, party or event.

**Features**

Features

• 400 watts, Class-D amplification

• 12” 2-way speaker design with 1.35” compression driver

• 2-input mixer

• Rugged, full grille design

• Signal Clip LED on back

• 2-band EQ

• Limiter with clip indicator

• Top and side handles

• 1-3/8" pole mount

• Ch 1 mic/line sensitivity switch with XLR and 1/4" jacks

• Ch 2 Line input with XLR and RCA jacks

• 1/8" Aux input for MP3 players

• XLR line level output to link speakers