**ST170**

**Active Ribbon Microphone**

**Brand**

Sterling

**Tagline**

Your Studio Sound

**What it is**

Sterling ST170 Active Ribbon Microphone

**EID#**

1500000051717

**MFID#**

J55794000000000

**GCID#**

113315683

**Possible Headlines**

• New Vintage Tone for Your Mic Toolbox

• Ribbon Smoothness with Modern Voicing

• Organic Sound from Modern Ribbon Technology

**Copy**

The Sterling Audio ST170 Active Ribbon Microphone brings a highly detailed, vintage-style tone to any recording environment with an ideal voicing for electric and acoustic guitars, drums, vocals and overhead/room. The active phantom powered design gives you the optimal output level to hit the tonal sweet spot of mic preamps, as well as ample ability to handle extra loud sources like guitar amps and drums. Its rich presence and warm bottom allow your mixes to come together quickly without heavy EQ. Includes SM5 metal shock mount and sturdy aluminum carry case. Requires phantom power.

**Features**

• Vintage tone for electric guitar, drums and other instruments

• Versatile Figure-8 pickup pattern

• Full frequency response: 20Hz – 20kHz

• Extreme volume handling: 132dB SPL

• Includes SM5 metal shock mount and aluminum case

• Requires phantom power

**Specifications**

Circuit Type: Active Ribbon

Polar Pattern: Figure-8

Capsule Design: 2-micron aluminum ribbon

Magnet: Rare earth neodymium

Frequency Response: 20Hz - 20kHz

Maximum SPL: 132dB SPL

Sensitivity: 16mV/Pa

Equivalent Noise: 22dB SPL A-Weighted

Typical Load Imp: >1000 Ohms

Output Source Imp: 200 Ohms Transformerless

Microphone Dimensions: 7.8” long, 1.4” max. diameter

Microphone Weight: 11.4 oz

Power Supply: +48V Phantom Power